Si3000/5000 Camera Driver Version 2.1

This installs the drivers for the Si3000/5000 camera and DsCap 3.92.

Start the Installation by double clicking your mouse on the batch file "setup.bat".
This will offer to install:

1. ICube Windows drivers from NET GmbH, compatible with the Si3000/5000 camera.  
2. The Si3000/5000 DirectShow camera driver, by EJC Associates. Required for making
   the camera compatible with DirectShow applications like DsCap, AmCap etc.
3. The DsCap DirectShow compatible camera viewer and capture application, by EJC Associates.

Three self extracting exe files will install in parallel. With each requiring your permission before it
will install. We suggest that you first agree to install the ICube drivers before continuing with
the rest of the installation.
 
The user is free to skip any part of the installation process. However, most will require the full
installation.

Once the ICube driver files have been extracted to your hard drive, we suggest that you connect the
camera USB cable to force Windows plug and play to detect the new hardware and install the Icube drivers.

Once the drivers have installed your will see the camera listed under "Imaging Devices" in Windows
Device Manager.

You may now continue with the remainder of the installation. i.e allow the installation of DsCap and
the Si3000/5000 driver by EJC Associates.

Please note that the installer for the Si3000/5000 driver will perform a cleanup of unneeded components
provided that it is installed after the ICube driver and after conecting the camera cable. This is the
reason for installing the ICube drivers first.

When the Si3000/5000 camera is first selected from a DirectShow application like DsCap, you will notice
its camera controls page is disabled and greyed out except for an edit box with the text
"Enter activation code". This is expecting you to enter the activation code supplied with your camera.
Type in the code, followed by the enter key. A correct entry will cause the edit box to disappear and
activate all the controls on the camera controls pages.

Please keep your activation code safe in case you need to reinstall at a future date. your camera
serial number is printed on the case and is always displayed on the Si3000/5000 camera controls page.
The serial number and the associated activation code are required if you require technical support from
EJC Associates.

Initially DsCap starts in Demo Mode, with the video canvas displaying "Please register DsCap to remove this
message". This message will appear until DsCap finds an activated Si3000/5000 camera.

Technical support is availabe from EJC Associates via the email address: support@ejc-associates.co.uk

Please provide the following information when applying.

1. Your name and address
2. Your camera serial number. This may be found with your camera and is always displayed on the
   DsCap camera controls page when the Si3000/5000 camera is selected and available.
3. The activation code that was bundled with your camera for unlocking the Si3000/5000 camera controls.
4. The version of DsCap installed.
